1. Install InfinityPlay and launch it.
2. Login to InfinityPlay(if you don’t have Goji account you can use username:**DENYS** with password:**qwe123ASD**)
3. Connect hardware to usb port
4. Open a setting page(small gear on top bar) then Inifinity & Belt Setup
5. Click on “Debug INFO” label on the left to open debug view
6. You can see there connection state and data from seed sensor/loadcells/belt
7. You can adjust resistance slider(if LED strip connected it will change color depending on a resistance value)